

Figure 5: The four figures above include the plots that were generated in the model where the efficiency was modeled using E= 1/Y.







Figure 6: The four figures above include the plots that were generated in the model where the efficiency was modified using the equation E=my+b.